**PRILOG I - TEHNIČKE SPECIFIKACIJE**

**APPENDIX I - TECHNICAL SPECIFICATIONS**

**ZA NABAVU STROJA, EVIDENCIJSKI BROJ NABAVE 03/2023/ZOSI**

**Stroj za obradu stretch folije ili jednakovrijedno**

**FOR THE PROCUREMENT OF MACHINER, PROCUREMENT REGISTRATION NUMBER 03/2023/ZOSI**

**Stretch film machine or equivalent**

*NAPOMENA/RTEMARK:*

*Za sve stavke navedene u tehničkim specifikacijama u kojima se možebitno traži ili navodi marka, norma te standardi, patent, tip ili određeno podrijetlo ponuditelj može ponuditi „jednakovrijedno“ svemu traženom ili navedenom.*

*For all items listed in the technical specifications in which the brand, norm and standards, patent, type or specific origin may be requested or specified, the bidder can offer "equivalent" to everything requested or specified.*

Ponuditelj obavezno popunjava stupac «Ponuđene specifikacije».

Ponuditelju je dozvoljeno popunjavanje tehničkih specifikacija upisujući točne karakteristike ponuđene robe.

**Ako nije drukčije navedeno, zahtjevi definirani tehničkim specifikacijama predstavljaju minimalne tehničke karakteristike koje ponuđeni predmet nabave mora zadovoljavatite se iste ne smiju mijenjati od strane Ponuditelja.**

**The bidder must fill in the "Offered specifications" column.**

The bidder is allowed to fill in the technical specifications by entering the exact characteristics of the offered goods.

**Unless otherwise stated, the requirements defined in the technical specifications represent the minimum technical characteristics that the offered procurement item must satisfy and may not be changed by the Bidder.**

| **Stavka** | **Tražene specifikacije** | **Ponuđene specifikacije** |
| --- | --- | --- |
| **Stretch film machine** | **Stroj za obradu stretch folije ili jednakovrijedno**-automatizirano prematanje stretch folije sa jumbo role na rolu folije-napon 3x400V-potrošnja energije 2,5kW-tlak zraka max 8 bara-učinkovitost 2 tone/h-maksimalna jumbo težin 50-70 kg-pričvrsne jezgre pneumatski-pritisak jezgre na središte osovina pneumatski-termalno odsijecanje-inverter za kontrolu brzine-jumbo podizni lift-signalni toranj**Stretch film machine or equivalent**-automated rewinding of stretch film from a jumbo roll onto a roll of film-power 3x400V-power consumption 2,5kW-air pressure max 8 bar-efficiency 2 tons/h-maximum jumbo weight 50-70 kg-fixing cores pneumatic-cores pressure to the central shaft pneumatic-cutting off thermal-speed control Inverter-jumbo lifting elevator-signal tower |  |

U \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_, \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

 ( mjesto/place ) (datum/date)

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ M.P.

*(ime i prezime i potpis osobe ovlaštene po zakonu za zastupanje gospodarskog subjekta)*

*(name and surname and signature of the person authorized by law to represent the economic entity)*